| **S/N** | **DETAIL** | **UNIT** | **MINIMUM REQUIREMENTS** | **TENDERER’S GUARANTEE** |
| --- | --- | --- | --- | --- |
|  | Name |  | Ready Board |  |
|  | Applicable Standards |  | IEC60050,  IEC60898-1  IEC61009-1 |  |
|  | Rated Voltage | V | 240 |  |
|  | Rated Frequency | Hz | 50 |  |
|  | Earth Leakage Circuit Breaker |  | 1 piece, 2 pole, 63A  With Overcurrent protection device |  |
|  | MCB |  | 3 pieces,  1-pole, 1\*25A, 1 pole, 2\*20A |  |
|  | Terminal |  | With separate PE and N bar |  |
|  | Socket Outlets | No. | 3 |  |
|  | Rating of Outlets with Switch 13A | A | 13 |  |
|  | Enclosure Material |  | Anti-flaming ABS |  |
|  | Degree of Protection |  | IP31 |  |
|  | Operating ambient temperature | 0C | -1 to 40 |  |
|  | Maximum humidity | % | 85 |  |
|  | Previous Type Test certificate to be provided with bid | Yes/No | Yes |  |
|  | Sample Test and Routine Test certificates to be provided on delivery | Yes/No | Yes |  |
|  | Quality Assurance certificate to be provide with bid | Yes/No | Yes |  |